The following performance information is based on Glastar N9079T
Taildragger configuration; 8.50 X 6 tires
Lycoming O360 A1A-normally aspirated 
Port/ polishing performed by LYCON;
 Estimated HP of 200-205; 9.0:1 C.R.
Propeller: DUC Cobra Black; 3-blade; 74”

Takeoff Rolls @ 60˚ F; 29.94 BP; estimated 3-4kt wind, Elev 2140’ [Calculated DA 2693’]
All runs with 180# Pilot, 16 - 19 gal fuel
15˚  Flaps – Avg  304’  [3 runs]     344	297	270
30˚  Flaps -Avg’  210’   [3 runs]     225	206	200

ROC easily 1200- 1500 fpm solo. I typically cruise at 125-130 kts
