1963 Comanche 250 N8165P sn 3420 (times approximate –flown regularly) This is an exceptionally nice Comanche:
As of 6/7/26:TT 3846: TSMOH by G&N 913.; Oil analyses in logs with every oil change since 2008; Digital logs and borescope images available
                     TSNew  Prop ( 3 blade McCauley)  954.7 hrs.
                     Annual done September 2025
                     IFR transponder/altimeter certification due 4/21/2027
[bookmark: Bookmark]AIRFRAME:               
	Paint done 2021 (9/10) - split base white and metallic gray with metallic black and emerald green accents
	Excellent glass and rubber, wing root seals replaced during repaint
	Speed mods – flap and aileron gap seals, wing root fairings, MLG speed spats, flap hinge fairings
	Large dorsal fin with integrated NACA fresh air intake
	1 piece windshield
	Polished spinner
	Stainless steel screws & fasteners
	Small nose wheel
	3 point strobes
	LED landing lights (Whelan G3 Parmetheus) with pulse mode
	120 gal (114 usable) with tip tanks and 3000 lb GW upgrade—approx 1200 nm no wind range
	Webco entry door upper latch
	New Plane Power 70 amp alternator installed 9/2023
	Concord AGM battery, new 2023
	Bogert battery box and copper cable
INTERIOR:
Custom  2-tone grey Cessna Citation leather done 2017 (9/10) in excellent condition – burn test certificates in logs
Color coordinated seat belts and shoulder harnesses all 4 seats
KingAir wemac fresh air vents
Rosen visors
Extra cabin insulation
Grey flat metal instrument panel with pilot & copilot 12V aux power jacks Cheyenne control wheels with PTT on both, A/P disconnect & altitude hold on pilot’s side
4 place headset jacks
Kennon heat screens
Cowl plugs
AVIONICS & INSTRUMENTS:
#1 nav com Garmin GTN 750 Xi WAAS with ADS-B traffic and weather, audio panel, installed 5/24
	Aspen 1000 Pro with AOA, synthetic vision, ADS-B weather, and traffic
	#2 nav com KX 155
	Bendix-King VOR-Loc-GS indicator (dual glide slopes)
	GTN 750audio panel with 4 place intercom and remote transponder control
	Bendix-King KN 62 DME with nav 1-2 switching
	S-Tec 50 A/P with altitude hold and GPSS/LOC steering
	Garmin GDL 69 XM weather receiver
	Garmin GTX 345 ADS-B in/out
	Vertical card mag compass
	406 mHz Ameri-King AK451-2D ELT — battery due 2027
	Backup vac AI on pilot’s side
	Pilot’s side turn coordinator
	Pilot’s side backup altimeter
	BNC panel jack for dedicated handheld outside antenna
	Davtron m800 clock
	JPI EDM 700 Engine analyzer and fuel flow with data download jack
	Electronics International volt/amp meter with low voltage and alternator failure warning lights
	Shadin fuel flow with total fuel, fuel remaining, gallons to destination, endurance (hours & minutes)
	Copilot instrumentation
		Digital electronic AI
		Backup Electric DG
		ASI
		2nd turn coordinator
		Sweep second hand clock
Instruments internally lit, plus accessory panel flood lights
Backup vacuum system
Carb ice detector with warning light
Electric aileron trim
Electric flaps
Complete parts and service manuals


Max payload with 90 gal. = 794 lbs; With 120 gal = 514 lbs
Flight plan TAS 160 Kts @ 13.5 gph; 114 gal approximate range 1200 nm with 1 hr reserve; 84 gal = 850 nm with 1 hr reserve
No known damage history; all logs, except for first 5 years - ’63-’68 - which have been reconstructed; all AD’s c/w
AdLog system.
Kept in heated hangar on aviation BatteryMinder with airframe interface

DISCLAIMER: The Seller provides the information herein to assist the Buyer in evaluating this aircraft. While every effort has been made to ensure accuracy, errors and omissions may occur. The Buyer is solely responsible for verifying all specifications, equipment, times, statuses, and conditions prior to closing. The Seller shall not be held liable for any discrepancies discovered after closing, and is not obligated to provide anything beyond what is expressly agreed upon. Aircraf, price is subject to change without notice and is subject to prior sale, withdrawal, or unavailability. No warranty, express or implied, is offered, and aircraft will sell as is, where is.


